How do I use the Elmo?
(note – picture from VCR or DVD will not play through the LCD panel in the cabinet)
Turn on LCD monitor in the top cabinet

See arrow #1

Turn on Elmo unit

See arrow #2

[image: image1.jpg]



On the Elmo control panel

· Press the MAIN/MODE button (#1) so that the SXGA light (#2) is on

· If showing something that is NOT a transparency, be sure the UPPER lights are on #3

· If using a transparency, try using the BASE light #4

You should see your display in the LCD monitor in the cabinet
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Turn on LCD Projection Unit

Press button #1 (green) to turn unit on

· Press RGB button #2 repeatedly until you see 

· RGB1 – for ELMO
on the classroom screen
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Manipulating the image

Use the AUTO FOCUS button #1 if your picture is not clear

Use the ZOOM buttons (TELE and WIDE) #2 to zoom in or out of your image
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