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Elmo and LCD monitor, top cabinet

-- this is the basic unit for showing overhead images

-- this unit also needs to be turned on the access the internet

To access the internet:

1. Turn on LCD monitor in the top cabinet 

2.Turn on Elmo unit

3. On the Elmo control panel press the RGB button (#1) 


4. Turn on the Computer


[image: image2.wmf]
use this remote (green button) to turn on the overhead projector

RGB button – for internet

Video button – for VCRs and DVDs
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For audio on the amplifier: Video 1 – VCR / Video 2 – internet / Video 3 – DVD

To use Elmo for overheads:

1. Turn on LCD monitor in the top cabinet

2. Turn on Elmo unit

3. On the Elmo control panel:


Press the MAIN/MODE button so that the SXGA light is on

· If showing something that is NOT a transparency, be sure the UPPER lights are on 
· If using a transparency, try using the BASE light 
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Press green button to turn overhead projector on

Press RGB button repeatedly until you see 

· RGB1 – for ELMO

on the classroom screen
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Manipulating the image

Use the AUTO FOCUS button if your picture is not clear

Use the ZOOM buttons (TELE and WIDE) to zoom in or out of your image
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BE VERY CAREFUL TO TURN EVERYTHING OFF WHEN FINISHED!

UNITS MAY OVERHEAT IN THE CLOSED CABINET
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